**Configure RGA IP Address**

The default serial settings for RGA are:

Baud rate: 115200

Data bits: 8

Parity: None

Stop bits: 1

Command to get IP address is:

pget IP-address

Commands to set IP address are:

pset assigned-IP xx xx xx xx (for example: 192 168 1 110)  
save

boot mon(this command will reboot the controller)

(after reboot, check if the IP is configured correctly)

pget IP-address